**PANEL:**

**AC POWER ELCB;**

**AC POWER RECEPTACLES;**

**AMPERE METER; HOUR METER; ENGINE INDICATOR; FUEL GAUGE; CURRENT REGULATOR; WELDING TERMINALS; START SWITCH;**

**MODE SELECTOR ------CC/CV**

**REMOTE SELECTOR REMOTE/LOCAL**

**IDLE CONTROL AUTO OFF**

**DUAL/SINGLE SELECTOR**

**EMERGENCY STOP**

**WIRE-FEEDER**

**REMOTE SOCKET**

Features:

Versatile welding and cutting partner for heavy construction;

Low-noise with 1500/1800rpm and KOVO P-noise solution;

Durable power, with Japan made Kubota V3300;

High efficiency, 500A DC welding and AC power simultaneously use;

Flux welding with wire-feeders;

Pipeline all position welding with dual welding output;

Maintenance-free, brushless design;

Safety warranty with Mitsubishi ELCB

WELDER AND GENERATOR WORK SIMUTANOUSLY

CC/CV OUTPUT COULING WIRE-FEEDER; 6-20KVA GENERATOR PLUS;

ECONOMICAL OPERATING COST WITH ECO KUBOTA ENGINE

DC Stick (SMAW)

Arc Gouging (CAC-A)

DC TIG (GTAW)

DC MIG (GMAW)

Flux cored (FCAW)

Specifications given herein are subject to change without notice

CAT. NO. DUV12-20170520

PRINTED IN 2017

|  |  |  |
| --- | --- | --- |
| **KOVO ENGINE DRIVEN WELDER EW500DST** | | |
| ***DC Welder*** | | |
| **Driven** | - | Direct Coupling |
| **Rated Output** | KW | 20 |
| **Rated Current** | DCA | 500-CC |
| DCA | 280A\*2-CC |
| DCA | 400A-CV\* |
| **Rated Voltage** | DCV | 40 |
| **Current Range** | DCA | 50-500 |
| **OCV** | DCV | 80 |
| **Duty Cycle** | % | 60 |
| **Type** | - | Rectified DC output type |
| **Applicable Electrode** | mm | 2.0-10.0 |
| ***Aux. Power*** | | |
| **Rated Output** | KVA | 6-20 |
| **Rated Voltage** | V | AC 127 /220 (AC220/380/415) |
| **Phase** | - | Three & Single |
| **Power Factor** | % | 80 |
| **Rate** | - | Continuous |
| ***ENGINE*** | | |
| **Model** | - | KUBOTA V3300 |
| **Type** | - | 4-cycle, water-cooled diesel engine |
| **Cylinder arrangement** | - | 4-L |
| **Total displacement** | cc | 3,318 |
| **Rated Output** | KW | 30.6 |
| **Speed** | rpm | 1,500 (1,800) |
| **Fuel** |  | Light diesel oil |
| **Start System** | - | Electric motor |
| **OTHER** | | |
| **Fuel Tank Capacity** | L | 68 |
| **Battery Capacity** | - | 12V-60AH |
| **Dimension (L×W×H)** | mm | 1850×806×1052 |
| **Net Dry Mass** | Kg | 960 |
| **Noise level** | dB | 67 |